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1. Wooden Pallet 1143mm x 1143mm x 130mm 
Wooden top planks: 1143L x 92W x 20H x 9 pcs
Wooden runners: 1143L x 38W x 90H x 4pcs
Wooden bottom planks: 1143L x 120W x 20H x 3 pcs
UOM: MM 
Material: Mixed Hardwood (selected MHW for prolong outdoor storage) 
Local SG Heat Treatment Required include 60 days warranty, IPPC stamp and certificate
Load weight: Min 3.8 MT / pallet 
Surface: S4S Smooth sawn all sides 
Weight: 25-30KG

Pallet marking : Company Abbreviation “XX” (Left of runner)
Pallet marking: Date “MM/YY” (Right of runner) 



2. Wooden Plywood 2311mm x 1143mm x 9mm 
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Weight: 10-12 KG
Material: BBCC plywood (BB-grade front face, CC-grade back face)
Local SG Heat Treatment Required include 60 days warranty, stamp and certificate

Stamp Requirements: SG IPPC Mark required on every single sheet of plywood 
Surface: 1 sided Red face, water resistance, another white face 

Moisture content: > 12% 

Glue: MR/E2 

With Sanding, closely filled inner fillings 

Note * Plywood inner filling required to be filled tightly, loose inner filling is not accepted 
Note * Plywood needs to be straight, delivered in wooden pallet base to ease unloading


3.Kubota plywood 900mm x 1040mm x 5.5mm (T)
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Weight: 5 KG
Material: BBCC plywood (BB-grade front face, CC-grade back face)
Local SG Heat Treatment Required include 60 days warranty, stamp and certificate

Stamp Requirements: IPPC Mark required on every single sheet of plywood
Surface: 1 sided Red face, water resistance, another white face

Moisture content : > 15% 

Glue: MR/E2 

No Sanding, hot pressing x 1 time  

Note * Plywood inner filling requires to be filled tightly, loose inner filling is not accepted


4.Wooden stick 2438.4mm x 88mm x 38mm 
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Weight: 10 KG
Material: Mixed Hardwood 
Local SG Heat Treatment Required include 60 days warranty, stamp and certificate

Stamp Requirements: IPPC Mark required on every timber stick 
Surface: Rip-Sawn S2S

Note * Timber needs to individually selected and wood need to be straight; bend wood will be rejected. 


5.Wooden Stick 782.8mm x 88.9mm x 38.1mm 
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Weight: 5 KG
Material: Mixed Hardwood 
Local SG Heat Treatment Required include 60 days warranty, stamp and certificate

Stamp Requirements: IPPC Mark required on every timber stick 
Surface: Rip-Sawn S2S

Note * Timber needs to individually selected and wood need to be straight; bend wood will be rejected.


6.Wooden stick 2550mm x 88mm x 38mm 
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Weight: 10-12 KG
Material: Mixed Hardwood 
[bookmark: _GoBack]Local SG Heat Treatment Required include 60 days warranty, stamp and certificate

Stamp Requirements: Every IPPC Mark required on every single timber stick 
Surface: Rip-Sawn S2S

Note * Timber needs to individually selected and wood need to be straight; bend wood will be rejected. 
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